[iface]
s_name_dev=ADSL / DIR 
s_language=Language
s_installcd=Install CD disk
s_viewmanual=View Manual
s_viewqig=View QIG
s_acrobat=Install Acrobat\n Reader
s_installddm=Install DDM
s_viewcd=View CD
s_quickinstall=Start
s_st1=1. Install Device
s_st2=2. Internet Setting
s_st3=3. Internet Connection
s_st4=
s_exit=Exit
s_next=Next >>
s_back=<< Back
s_yes=Yes
s_no=No
s_ok=Ok
s_cancel=Cancel
s_open=Open
s_custom_settings=Adjusted manually
s_skip=No
s_repeat=Yes


s_help1_page1=Please connect the power cord to the appropriate connector on the device and into a power outlet
s_help2_page1=Before clicking Next, make sure that the Power LED on the front panel is lit
s_help1_page2=Connect the cable from the Ethernet-LAN-port device and Ethernet-port on your computer
s_help2_page2=Please make sure the LAN light is lit before clicking Next
s_help1_page3=Connect the Ethernet-cable provider to the WAN-port (Internet) device. Or connect the micro filter / splitter (available on some models) to the telephone socket. With the gray cable to connect the DSL-port device to a DSL-jack microfilter / splitter
s_help2_page3=Please make sure that the WAN light or DSL light is lit before clicking Next
s_help1_page_netiface=Choose the network interface of the computer that is currently connected to a device
s_stat_page_netiface=Choose the network adapter
s_help1_page_provider=Please select your provider from the list and then click Next
s_help2_page_provider=For the device did not match any configuration file
s_stat_page_provider=Choice of provider
s_help1_page_change_account=Selected service provider requires that the default password to access the device has been modified\n\nPlease enter the new password to access the device
s_stat_page_change_account=Change the password to access the device
s_help1_page_wifi=Customize WI-FI
s_stat_page_wifi=Customize WI-FI
s_help1_page_mer_static=Please specify the information provided by provider
s_ip_addr_page_mer_static=IP address
s_ip_mask_page_mer_static=Subnet Mask
s_gw_page_mer_static=Default Gateway
s_dns1_page_mer_static=Preferred DNS-server
s_dns2_page_mer_static=Alternative DNS-server
s_help1_page5=Please have the information provided by your ISP to configure the Internet connection.
s_help2_page5=The device was found and verified.\n\nTo continue, click Next.
s_stat_page5=To check your connection devices
s_authorize_page5=Authorization
s_stat_page_network_settings=Configuration provider
s_help1_page_finish=Congratulations!!!\n\nProcess installation completed - access to the internet set up
s_help2_page_finish=Protsess installation completed!!!
s_type_connection=Type connection
s_type_connection_pppoe=Internet (PPPoE)
s_type_connection_ipoe=Internet (IPoE)
s_type_connection_custom_settings=Please enter your information for the fields listed below. If you do not know what point, then click Next
s_select_manual=Please select your divice


s_wait=Please wait...
s_wait_status_provider=Is to construct a list
s_wait_status_page_netifaces=Searching for network interfaces
s_wait_status_page5=To check your connection devices
s_wait_change_password=Changing your password on the device
s_wait_status_page_network_settings=Device Setup
s_wait_for_reprogramming=Upgrading Software
s_wait_restart=Reboot the device
s_wait_restore_default=Reset to factory settings
s_wait_save_config=Save configurations
s_wait_create_pvc=Setting
s_wait_remove_wans=Removal of the existing configuration of WAN interfaces
s_wait_create_groups=Create a Group
s_wait_remove_groups=Removal of the existing groups of interfaces
s_wait_settings_lan=Setting
s_wait_create_static_route=Creating a static route on the modem:
s_wait_set_default_gateway=Assigning a default gateway
s_wait_get_data_wifi=Getting the settings for Wi-Fi
s_wait_send_data_wifi=Sending parameters Wi-Fi device
s_wait_create_vlan=Create VLAN
s_wait_remove_vlans=Remove existing VLAN
s_wait_adapter=Changing the network adapter settings
s_wait_internet_connection=Checking Internet Connection
s_wait_settings_phone=Phone settings

s_vpi=Vpi
s_vci=Vci
s_adapter_name=Network adapter name
s_adapter_ip_addr=IP address
s_adapter_ip_mask=Netmask
s_adapter_id=ID
s_isp_region=Region
s_isp_name=ISP Name
s_isp_description=Description
s_config=Configuration of
s_login_prompt=Please, enter username and password for access to your device.
s_username=Username
s_password=Password
s_repassword=Confirm Password:
s_login=Username:
s_phone=Phone
s_number_phone=Phone number
s_wireless_title=Customize WI-FI
s_wireless_status=Status
s_wireless_channel=Channel
s_wireless_ssid=SSID
s_wireless_encrypt=Encryption Type
s_wireless_key=Key

s_ch_wirelessStatus_on=On
s_ch_wirelessStatus_off=Off

s_sel_item_recommended=(recommended)
s_sel_item_not_encrypt=without encryption (not recommended)
s_sel_item_wep64=WEP (64-bit)
s_sel_item_wep128=WEP (128-bit)
s_sel_item_wpa=WPA
s_sel_item_wpa2=WPA2
s_sel_item_psk=PSK
s_sel_item_wpapsk=WPA-PSK
s_sel_item_wpa2psk=WPA2-PSK
s_sel_item_wpa_wpa2=WPA-WPA2
s_sel_item_wpapsk_wpa2psk=WPA-PSK/WPA2-PSK

s_hint_wep64=Enter 5 ASCII characters or 10 hexadecimal digits.
s_hint_wep128=Enter 13 ASCII characters or 26 hexadecimal digits.
s_hint_wpa=Enter the IP-address of the RADIUS server.
s_hint_wpa2=Enter the IP-address of the RADIUS server.
s_hint_psk=
s_hint_wpapsk=WPA PSK key length should be 8 to 63 ASCII characters or 64 hexadecimal digits.
s_hint_wpa2psk=WPA PSK key length should be 8 to 63 ASCII characters or 64 hexadecimal digits.
s_hint_wpa_wpa2=Enter the IP-address of the RADIUS server.
s_hint_wpapsk_wpa2psk=WPA-PSK/WPA2-PSK key length should be 8 to 63 ASCII characters or 64 hexadecimal digits.

s_stb_title1=Service
s_stb_title2=Internet
s_stb_title3=IPTV
s_config_stb=Setting STB
s_config_stb2=Setting STB
s_servicename=Service
s_filial=Branch
s_country=Country
s_provider=Provider
s_mess_usbdriverinstallok=USB драйвер успешно установлен. Отключите устройство от USB порта компьютера и подключите вновь. В правом нижнем углу экрана появятся системные сообщения об обнаружении и установке нового оборудования. После их исчезновения нажмите кнопку "Ок" для закрытия этого окна и продолжения работы утилиты настройки.
s_link_megaman=User instructions for setting up the modem \nD-Link DSL-2500U/BRU/D for the network U-tel
s_winpppoe_cfg=Setting Connection
s_winpppoe_cr=Create Connection
s_check_exist_pppoe=Checking for PPPoE
s_check_status_pppoe=Checking the status of PPPoE
s_settings_vlan_id=Enter VLAN ID for
s_vlan_id=VLAN ID
s_change_ports_for_vlan=Select ports for

s_dap_mode=Work mode
s_dap_access_point=Access point
s_dap_router=Router

[EMessages]
e_no_adapters_found=The application has not found any working network adapter on this computer.\nPlease, check up the following:\n\n1. The power adapter is connected to your modem and an electrical outlet.\n2. Your modem's Ethernet cable is properly connected to your computer.\n3. Network card is properly installed in your computer.
e_no_device_found=The application has not found your modem.\nPlease, check up the following:\n\n1. The power adapter is connected to your modem and an electrical outlet.\n2. Your modem's Ethernet cable is properly connected to your computer.\n3. Network card is properly installed in your computer.
e_no_fw_found=Error! There is no firmware file.
e_login_failed=Error! Username or password is wrong!
e_connection_error=There was an error during data recieving from the device.\n\nApplication cannot be continued.
e_unsupported_device=Error! Connected device unsupported.
e_update_failed=Firmware update failed.\nThe current version will be used.
e_update_none=Firmware is not found, sew the device manually and restart the application
e_adsl_down=Please check the DSL cable is securely connected and the modem is fully operational.
e_providersini_error=Reading error of ISP profile.\n
e_pwd_len=The password should be at least four characters
e_pwd_incorrect=The password and confirmation is not identical.
e_http_error=There was an error at data transmission to the device.\n\nApplication cannot be continued.
e_prov_gateway_down=Access error to Internet Service Provider network.\nADSL-router cannot establish connection with default gateway of your ISP.\n\nThe possible reasons:\n -Malfunctions on the communication line or in the equipment of the provider.\n -The information provided by your ISP is incorrectly specified.
e_cannot_create_win_pppoe_connection=Sorry. The application cannot create connection for Internet access.\nYour modem has been adjusted in a bridge mode. Please, address to technical support service for help.
e_incorrect_wireless_ssid=Incorrect SSID
e_incorrect_wireless_security_key=Incorrect key
e_incorrect_data=Incorrect data
e_field_empty=Fill in all fields
e_caption_error=Error
e_caption_info=Help
e_incorrect_wireless_radius_server_ip_address=Incorrect RADIUS Server IP Address!
e_incorrect_servicename=Select a service!
e_incorrect_swver_lp=This version does not support changing the password to access the device.
e_usb_driver_run=Unable to install the driver. Disconnect the device from the USB port of your computer, connect again and run the setup utility.
e_auth_error=An error occurred when connecting to the ISP’s server. \nDo you want to reconfigure the device?
e_internet_connection_error=Internet connection is available. \nDo repeat adjustment of the device?
e_adsl_cable_disconnected=It’s not possible to check the Internet connection as the phone cable is not connected to the modem.
e_no_free_ports=No ports available
e_vlan_id_busy=VLAN ID is unavailable. Please enter another VLAN ID
e_vlan_ports_not_check=No port is selected

[confirm]
fw_update=It is necessary to update the software of your modem.\n\nPress "OK" to start updating.\nPress "Cancel" to exit.
fw_usbdriver=If your device - DSL-2520U, and it is connected to the USB port on your computer for normal operation of the configuration utility to install a driver for this device. Install the driver Yes / No?
fw_info_for_user=fw_info_for_user