### Template to Provision Termination Pointers and Cross Connection using TL1

- Example - Overview
- Making it Work
- Sample Output

Example - Overview

The template (CrossConnect.xml) uses the TL1 Protocol, to provision the termination pointers and cross-connections for the DS0 resources on a TDM device. Before a DS0 cross connection is created, the following two tasks are performed using the <ConfigTask> tag.

- Provisions each resource (source and the destinataion card) to be used in the cross-connection.
- Create cross connection between the source and the destination cards in the TDM Device

Making it Work

> Prerequisite

- The host under test should be a TL1 device
- Cross Connect feature should be supported by the device

Invoking the template

You can modify the template CrossConnect.xml in <Web NMS Home>/provisioningtemplates directory, for specific requirements. To invoke the template, you can choose one of the following methods.

- Invoking using Web NMS Client
- Invoking using Batch/Shell files
- Invoking using Applet Client

Invoking using Web NMS Client

Once a template is defined, it can be invoked from the Web NMS Client using the Provisioning node. From the Provisioning node of Web NMS Client, select the "Templates" menu option. This displays the provisioning templates available in <Web NMS Home>/provisioningtemplates directory. Select the CrossConnect template, to invoke the same.

Invoking using Batch/Shell script files

After starting the Web NMS Server, execute the file CrossConnect.xml using OpenTemplate.bat/.sh file in <Web NMS Home>/provisioningtemplates directory. From the UI displayed, specify the values for the parameters to view and invoke the template.

Invoking using Applet Client

To invoke the provisioning templates using applet client,

- From the browser type http://<hostname>:9090/html/TemplateTesterApplet.html
- An applet will be instantiated, from which the name of the template can be chosen
- Choose the template CrossConnect.xml, to view the template

Sample Output