

|  |  |
| --- | --- |
| **AP Version:** | 1.3 |
| **Published Date:** | 2013/05/15 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.3 | 2012/12/17 | DNR-326 | A2 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

MINIMUM SYSTEM REQUIREMENTS

OS Support

+ Windows XP SP2, Vista or 7 (32bit)

+ Web browser - Internet Explorer v7 to v9

+ Computer with:

- Pentium 4 – 2.4 GHz

- 512MB RAM

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.3 | 1. Modify product name of DNR-322L in Setup. Exe (AP): 2-bay professional  NVR |
|  |  |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.3 |  |
|  |  |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
|  |  |
|  |  |
|  |  |

# Related Documentation:

* User Manual
* Datasheet

# Note:

* Please refer to Camera Support List in PMD system.