;****************************************************************************************
;
; rt2870.inf
;
;   This installation script supports Windows 2000 & XP for the
;   Ralink RT2870 series USB Wireless LAN Card.
;
;   Copyright (c)2002-2011 , Ralink Technology Corp., All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %D-Link%
Compatible      = 1
DriverVer       = 10/11/2012, 5.00.01.0000
CatalogFile     = rt2870.cat            ;for WHQL certified

[ControlFlags]
;***********Ralink 802.11 n board  ***********
ExcludeFromSelect = *

[Manufacturer]
%D-Link%        = D-Link
[D-Link]
; DisplayName               Section                        DeviceID
; -----------               -------                        --------
%D-Link_3C09.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C09
%D-Link_3C11.DeviceDesc%    = RTWLANH_C2.ndi,              USB\VID_07D1&PID_3C11
%D-Link_3C13.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C13
%D-Link_3C0A.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C0A
%D-Link_3C0B.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C0B
%D-Link_3C0D.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C0D
%D-Link_3C0E.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C0E
%D-Link_3C0F.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C0F
%D-Link_3C15.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C15
%D-Link_3C16.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_07D1&PID_3C16
%D-Link_3C17.DeviceDesc%    = RTWLAN_C5.ndi,               USB\VID_07D1&PID_3C17
%D-Link_3C20.DeviceDesc%    = RTWLAN_C2_single.ndi,        USB\VID_2001&PID_3C20
%D-Link_3C21.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_2001&PID_3C21
%D-Link_3C22.DeviceDesc%    = RTWLAN_C2_single.ndi,        USB\VID_2001&PID_3C22
%D-Link_3C23.DeviceDesc%    = RTWLAN_C2_single.ndi,        USB\VID_2001&PID_3C23
%D-Link_3C24.DeviceDesc%    = RTWLAN_C2.ndi,               USB\VID_2001&PID_3C24
%D-Link_3317.DeviceDesc%    = RTWLAN_C2_single.ndi,        USB\VID_2001&PID_3317

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RTWLAN.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANSB.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANDR.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, RemoveFlag.reg, CoInstOpt_DisableN.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANSD.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, CoInstOpt_DisableN.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, LinkSpeedStatus.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANG.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANRG.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANRGL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg, LinkSpeedStatus.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANH.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, IEEE80211H_SET.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANHC.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, IEEE80211H_SET.reg, CarrierDetect.reg, SmartScan.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, SmartScan.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_Az.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, RemoveFlag.reg, CoInstOpt_DisableN.reg, LinkSpeedStatus.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_Abo.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, InitChn14Disabled.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C1.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, Customer1.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, Customer2.reg, ChannelMode.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C2_single.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, IEEE80211H.reg, AdhocN.reg, Customer2.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANH_C2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, IEEE80211H_SET.reg, Customer2.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C3.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, RemoveFlag.reg, CoInstOpt_DisableN.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C4.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg, BTCoexist.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C4.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, BTCoexist.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C5.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, Customer2.reg, BTCoexist.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C6.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, BTCoexist.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C7.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C7L.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg, Feature.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C7DCh14.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand_DisCh14.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg, InitChn14Disabled.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

[cisco_ctv1w.ndi.NT]
AddReg                  = Common.reg, RTUSB_CTV1W.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, SmartScan.reg, BaldEagle.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT_CTV1W.CopyFiles

[RTWLAN_C9.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, LinkQualitySetting.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C10.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, NotProhibitTKIPonHT.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_C11.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, BTCoexist.reg, WepConnectCheckEncry.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C12.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, AdhocN.reg, PsControl.reg, WirelessModeSwitch.reg, RoamingDef_medium.reg, BackgroundScan.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN_C13.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, PsControl.reg, TssiPatchForAntennaVariation.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

[RTWLAN_LED2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, Led2.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, TxBf.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C1.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, TxBf.reg, LinkSpeedStatusRxDynamicRate.reg, TxRxConfigByRegistry.reg, WirelessModeSwitch.reg, MulticastRateAutoSelected.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C2.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg, TxBf.reg, WirelessMode_BGN.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C3.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, TxBf.reg, PsControl.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C4.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, TxBf.reg, PsControl.reg, StreamMode.reg, AdTxPwrForFCCTest.reg, IEEE80211H_SET.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C5.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, TxBf.reg, PsControl.reg, LinkSpeedStatusRxDynamicRate.reg, TxRxConfigByRegistry.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

[RTWLANR_3573_C6.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, TxBf.reg, PsControl.reg, CustomizedPowerMode.reg, CarrierDetect.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

[RTWLANR_7650.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, IEEE80211H.reg, AdhocN.reg, RemoveFlag.reg, PsControl.reg, TxBf.reg, Vht.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles

; NT services sections
[RTWLAN.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANSB.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANDR.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANSD.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANL.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANG.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANRG.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANRGL.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANH.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANHC.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANS.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_Az.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_Abo.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C1.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C2.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C2_single.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANH_C2.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C3.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C4.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C4.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C5.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C6.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C7.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C7L.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C7DCh14.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[cisco_ctv1w.ndi.NT.Services]
AddService              = CTV1W, 2, CTV1W.Service, cisco_ctv1w.EventLog

[RTWLAN_C9.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C10.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_C11.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C12.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_C13.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN_LED2.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C1.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C2.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C3.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C4.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C5.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_3573_C6.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR_7650.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************
[RTWLAN.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANSB.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANDR.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANSD.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANL.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANG.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANRG.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANRGL.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANH.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANHC.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANS.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_Az.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_Abo.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C1.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C2_single.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANH_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C3.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C4.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C4.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C5.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C6.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C7.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C7L.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C7DCh14.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[cisco_ctv1w.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C9.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C10.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_C11.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C12.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_C13.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN_LED2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C1.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C3.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C4.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C5.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_3573_C6.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR_7650.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                            CurProfile,      0,""
HKR, Default,                     CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Auto Reconnect Mode
;
HKR, ,                            AutoReconnect,   0, "1"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                            ShowHiddenSSID,  0, "0"   ; 0=disable(default), 1=enable

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; CCX drastic roaming use
;
HKR, ,                            CCXPktLossLimitTime,    0, "30"

;
; CCX Dbm offset
;
HKR, ,                            CCXDbmOffset,    0, "4"

;
; CCX VO/VI Drop Period, 3 or 5 is recommanded
;
HKR, ,                            CACDropPeriod,    0, "0"

;
; CCX VO/VI Drop Criteria
;
HKR, ,                            CACDropCriteria,    0, "1700"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable patch for pass wifi 11n draft
;
HKR, ,                            TGnWifiTest,     0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,  0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; CarrierDetect
;
HKR, ,                            CarrierDetect,   0, "0"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,0, "0"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"

;
; DirectMode
;
HKR, ,                            DirectMode,      0, "0"

;
; RDG
;
HKR, ,                            RDG,             0, "1"

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,0, "1"

;
; Link Speed Status
;
HKR, ,                            LinkSpeedStatus, 0, "0"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,        ParamDesc,       0, %SmartScan%
HKR, NDI\params\SmartScan,        type,            0, "enum"
HKR, NDI\params\SmartScan,        default,         0, "0"
HKR, NDI\params\SmartScan\enum,   0,               0, %Disable%
HKR, NDI\params\SmartScan\enum,   1,               0, %Enable%

;
; AdhocN40MHzAllowed
;
HKR, ,                            AdhocN40MHzAllowed,0, "0"

;
; WSC Version2 
HKR, ,                            WSCVersion2,     0x00010001, 0x00000020

;
; WSC 2.0 Testbed for some test items. 
HKR, ,                            WSC20Testbed,     0x00010001, 0x0000000C

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, %PSPXlink%
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, %Disable%
HKR, NDI\params\PSPXlink\enum,    1,               0, %Enable%

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Fast Roaming Sensitivity
;
HKR, ,                                  FastRoamingSensitivity,    0, "0"
HKR, NDI\params\FastRoamingSensitivity,              ParamDesc,    0, %FAST_ROAMING_SENSITIVITY_STR%
HKR, NDI\params\FastRoamingSensitivity,              Type,         0, "enum"
HKR, NDI\params\FastRoamingSensitivity,              Default,      0, "0"
HKR, NDI\params\FastRoamingSensitivity,              Optional,     0, "0"
HKR, NDI\params\FastRoamingSensitivity\enum,         "0",          0, %DISABLE_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "1",          0, %LOWEST_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "2",          0, %MEDIUM_LOW_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "3",          0, %MEDIUM_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "4",          0, %MEDIUM_HIGH_STR%
HKR, NDI\params\FastRoamingSensitivity\enum,         "5",          0, %HIGHEST_STR%

;
; Block ACK settings
;
HKR, ,                            BACapability,    0x10001, "0x0b034040"
HKR, Default,                     BACapability,    0x10001, "0x0b034040"

;
; Wifi Direct settings
;
HKR, ,                            WifiDirectControl,	0x10001, "0x803f8078"
HKR, Default,                     WifiDirectControl,	0x10001, "0x803f8078"

;
; P2P Reinforced ACK check
;
HKR, ,                            P2PAckCheck,    0, "1"
HKR, Default,                     P2PAckCheck,    0, "1"

;
; Enable P2P Video Boost within P2P Group
;
HKR, ,                            P2PVideoBoost,      0, "0"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting, 0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting, 0x10001, "0x2ba15"

;
; Rssi Delta
;
HKR, ,                            RssiDelta,       0, "6"

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                           SSID,            0, %SSID_DEF_STR%
;HKR, Default,                    SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,            ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,            type,            0, "edit"
;HKR, NDI\params\SSID,            limitText,       0, "32"
;HKR, NDI\params\SSID,            default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, %LocalNetworkAddress%
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""
HKR, NDI\params\Networkaddress,   optional,        0, "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, %PSMode%
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, %CAM%
HKR, NDI\params\PSMode\enum,      1,               0, %MAXPSP%

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                            AuthenType,      0, "0" ; Open System
HKR, Default,                     AuthenType,      0, "0"
                                  
;                                 
; Encryption                      
;                                 
HKR, ,                            Encryption,      0, "1" ; Disable
HKR, Default,                     Encryption,      0, "1"
                                  
;                                 
; WEP Keys Length                 
;                                 
HKR, ,                            WEPKeyLen,       0, "0"
HKR, Default,                     WEPKeyLen,       0, "0"
                                  
;                                 
; WEP Key to use                  
;                                 
HKR, ,                            WEPKeyUse,       0,"1"
HKR, Default,                     WEPKeyUse,       0,"1"
                                  
;                                 
; WEP Key1                        
;                                 
HKR, ,                            WEPKey1,         0,""
HKR, Default,                     WEPKey1,         0,""
                                  
;                                 
; WEP Key2                        
;                                 
HKR, ,                            WEPKey2,         0,""
HKR, Default,                     WEPKey2,         0,""
                                  
;                                 
; WEP Key3                        
;                                 
HKR, ,                            WEPKey3,         0,""
HKR, Default,                     WEPKey3,         0,""
                                  
;                                 
; WEP Key4                        
;                                 
HKR, ,                            WEPKey4,         0,""
HKR, Default,                     WEPKey4,         0,""
                                  
;                                 
; Reposit Bssid List              
;                                 
HKR, ,                            BssidRepositTime,0, "90"
                                  
[RemoveFlag.reg]                  
HKR, ,                            SafelyRemoveOff, 0, "1"
                                  
[IEEE80211H.reg]
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

[IEEE80211H_SET.reg]                  
HKR, ,                            IEEE80211H,      0, "1"
                                  
[CarrierDetect.reg]               
HKR, ,                            CarrierDetect,   0, "1"
                                  
[SmartScan.reg]                   
HKR, ,                            SmartScan,       0, "1"

[BackgroundScan.reg]
HKR, NDI\params\SmartScan,        ParamDesc,       0, %BackgroundScan%
HKR, NDI\params\SmartScan\enum,   0,               0, %ALLOW%
HKR, NDI\params\SmartScan\enum,   1,               0, %DISALLOW%

[AdhocN.reg]
;
; AdhocNMode
;
HKR, ,                            AdhocNMode,      0, "0"
HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
HKR, NDI\params\AdhocNMode,       type,            0, "enum"
HKR, NDI\params\AdhocNMode,       default,         0, "0"
HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable%

[PsControl.reg]
;
; Power Saving Control
;
HKR, ,                            PSControl,       0x00010001, 0x00000001

[SingleBand.reg]
;
; 2.4G Band
;
HKR, ,                                   CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,           ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,           type,               0, "enum"
HKR, NDI\params\CountryRegion,           default,            0, "0"
HKR, NDI\params\CountryRegion\enum,      0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,      1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,      2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,      3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,      4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,      5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,      6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,      7,                  0, %CountryRegion24G_7%

[DefaultBand.reg]
;
; 2.4G Band
;
HKR, ,                                   CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,           ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,           type,               0, "enum"
HKR, NDI\params\CountryRegion,           default,            0, "0"
HKR, NDI\params\CountryRegion\enum,      0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,      1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,      2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,      3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,      4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,      5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,      6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,      7,                  0, %CountryRegion24G_7%

;
; 5G Band
;
HKR, ,                                   CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,      ParamDesc,          0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand,      type,               0, "enum"
HKR, NDI\params\CountryRegionABand,      default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum, 0,                  0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum, 1,                  0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum, 2,                  0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum, 3,                  0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum, 4,                  0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum, 5,                  0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum, 6,                  0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum, 7,                  0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum, 8,                  0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum, 9,                  0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum, 10,                 0, %CountryRegion5G_10%
HKR, NDI\params\CountryRegionABand\enum, 11,                 0, %CountryRegion5G_11%
HKR, NDI\params\CountryRegionABand\enum, 12,                 0, %CountryRegion5G_12%
HKR, NDI\params\CountryRegionABand\enum, 13,                 0, %CountryRegion5G_13%
HKR, NDI\params\CountryRegionABand\enum, 14,                 0, %CountryRegion5G_14%
HKR, NDI\params\CountryRegionABand\enum, 15,                 0, %CountryRegion5G_15%
HKR, NDI\params\CountryRegionABand\enum, 16,                 0, %CountryRegion5G_16%

[SingleBand_DisCh14.reg]
;
; 2.4G Band
;
HKR, ,                                   CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,           ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,           type,               0, "enum"
HKR, NDI\params\CountryRegion,           default,            0, "0"
HKR, NDI\params\CountryRegion\enum,      0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,      1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,      2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,      3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,      6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,      7,                  0, %CountryRegion24G_7%

;*******************************************************************************************
; Customer Request
;*******************************************************************************************

[Customer1.reg]
;
; Customer request for Allied 
;
; Vendor Description
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%

; WPS Device Name
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%

[Customer2.reg]
;
; D-Link Request
;
; WMMCapable
HKR, ,                            WMMCapable,      0, "1"
; Show Hidden SSID in Site Survey Page
HKR, ,                            ShowHiddenSSID,  0, "1"   ; 0=disable(default), 1=enable
; Enable TX Burst
HKR, ,                            TXBurst,         0, "1"
; DLSCapable
HKR, ,                            DLSCapable,      0, "1"

[BTCoexist.reg]
HKR, ,                BTSoftwareOn,      0, "0"
HKR, ,                BTConfiguration, 0x00010001, 0x380004fd

[LinkSpeedStatusRxDynamicRate.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "2"

[LinkSpeedStatus.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "1"

[LinkQualitySetting.reg]
;
;LinkQualitySetting
;
HKR, ,                            LinkQualitySetting, 0x00010001, "0x51"

[GainProSpeed.reg]
HKR, ,                            GainProSpeed, 0x00010001, 0x00000300 

[InitChn14Disabled.reg]
;
; Disable Channel 14 for JP
;
HKR, ,                            InitChn14Disabled,0,"1"

[CoInstOpt_DisableN.reg]
;
; RaCoInstaller Options
;
; CoInstaller Options for Azurewave, MSI
HKR, ,                            RaCoInstOpt,     0,"00101111"
HKR, ,                            CountryWirelessMode,     0x00010001, 0x00001000 

; WirelessMode
HKR, ,                            WirelessMode,    0, "3"

[BaldEagle.reg]
;
; Bald Eagle Mechanism
;
HKR, ,                            BaldEagleSSID, 0, %BaldEagle_SSID%

[Led2.reg]
;
; Led Configuration
;
HKR, ,                            LedCfg,  0, "1"   ; 0=firmware(def), 1=asic

[Feature.reg]
HKR, ,                FeatureSetting, 0x00010001, 0x1

[TxBf.reg]
;
; ETxBfEn
;
HKR, ,                            ETxBfEn,		0,	"1"

;
; ETxBfTimeout
;
HKR, ,                            ETxBfTimeout,	0,	"40000"

;ss
; ETxBfNonCompressedFeedback
;
HKR, ,                            ETxBfNonCompressedFeedback,	0,	"0"

[Vht.reg]
;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x8F21B"
HKR, Default,                     TransmitSetting,      0x10001, "0x8F21B"

; WirelessMode
HKR, ,                            WirelessMode,    0, "11"

[TxRxConfigByRegistry.reg]
;
;TxRxConfigByRegistry
;
HKR, ,                            TxRxConfigByRegistry,	0,	"1"

[MulticastRateAutoSelected.reg]
;
;MulticastRateAutoSelected
;
HKR, ,                            SoftAPForceMulticastRate, 	0,	"11000000"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInst.dll,ClassCoInstaller"

[NotProhibitTKIPonHT.reg]
;
; Not ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,0, "0"

[WepConnectCheckEncry.reg]
;
; Check Encry of AP when setting WEP connection
;
HKR, ,                            WepConnectCheckEncry,0, "1"

[WirelessMode_BGN.reg]
; WirelessMode BGN Only
HKR, ,                            RaCoInstOpt,     0,"00101111"
HKR, ,                            CountryWirelessMode,     0x00010001, 0x00001110

HKR, ,                            WirelessMode,    0, "9"

[WirelessModeSwitch.reg]
; 2.4G/5G Switch
HKR, ,                              RaCoInstOpt,     0,"00101111"
HKR, ,                              WirelessMode,    0, "5"
HKR, NDI\params\WirelessMode,       ParamDesc,       0, %WirelessMode%
HKR, NDI\params\WirelessMode,       type,            0, "enum"
HKR, NDI\params\WirelessMode,       default,         0, "5"
HKR, NDI\params\WirelessMode\enum,  5,               0, %WirelessModeBoth%
HKR, NDI\params\WirelessMode\enum,  9,               0, %WirelessMode24G%
HKR, NDI\params\WirelessMode\enum,  8,               0, %WirelessMode5G%

[RoamingDef_medium.reg]
HKR, ,                                FastRoamingSensitivity,    0, "3"
HKR, NDI\params\FastRoamingSensitivity,              Default,    0, "3"

[TssiPatchForAntennaVariation.reg]
HKR, ,                            TssiPatchForAntennaVariation,  0, "1"

[StreamMode.reg]
HKR, ,                            StreamMode,         0, "1"

[AdTxPwrForFCCTest.reg]
HKR, ,                            AdTxPwrForFCCTest,  0, "1"

[CustomizedPowerMode.reg]
HKR, ,                            CustomizedPowerMode,  0, "1"

[ChannelMode.reg]
HKR, ,                                 ChannelMode, 0, "1"
HKR, NDI\params\ChannelMode,    ParamDesc,          0, %CHANNEL_MODE%
HKR, NDI\params\ChannelMode,    type,               0, "enum"
HKR, NDI\params\ChannelMode,    default,            0, "1"
HKR, NDI\params\ChannelMode\enum,0,                 0, %ChannelMode_0%
HKR, NDI\params\ChannelMode\enum,1,                 0, %ChannelMode_1%
HKR, NDI\params\ChannelMode\enum,2,                 0, %ChannelMode_2%

;
; Remove registry
;
[RegRemove.delReg]
; Remove CountryRegion
HKR, NDI\params\CountryRegion
HKR, NDI\params\CountryRegionABand

; Remove IEEE80211H
HKR, NDI\params\IEEE80211H

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
NT_CTV1W.CopyFiles      = 12
CoInstaller.CopyFiles   = 11

[NT.CopyFiles]
rt2870.sys                   ; NT Installation

[NT_CTV1W.CopyFiles]
CTV1W.sys,rt2870.sys,,2	     ; NT Installation

[CoInstaller.CopyFiles]
RaCoInst.dll
RaCoInst.dat

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2870.sys              = 1
RaCoInst.dll            = 1
RaCoInst.dat            = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2870"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[RTUSB_CTV1W.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "CTV1W"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2870.sys
LoadOrderGroup              = NDIS

[CTV1W.Service]
DisplayName                 = %CTV1W.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\CTV1W.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[cisco_ctv1w.EventLog]
AddReg=CTV1W.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2870.sys"
HKR, , TypesSupported,   0x00010001, 7

[CTV1W.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\CTV1W.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Local MAC Network Address"
PSMode                      = "Power Saving Mode"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc support 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensitivity" 
DISABLE_STR                 = "6.Disable"
LOWEST_STR                  = "5.Lowest"
MEDIUM_LOW_STR              = "4.Low"
MEDIUM_STR                  = "3.Medium"
MEDIUM_HIGH_STR             = "2.High"
HIGHEST_STR                 = "1.Highest"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Traditional Chinese 
;*******************************************************************************************
[Strings.0404]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "無線裝置 開/關"
Disable                     = "停用"
Enable                      = "啟用"
CountryRegion24G            = "頻道代碼 (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "頻道代碼 (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒體/遊戲環境"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "網路實體位址"
PSMode                      = "省電模式"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "隨意網路支援 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

FAST_ROAMING_SENSITIVITY_STR = "漫遊靈敏度" 
DISABLE_STR                 = "6.停用"
LOWEST_STR                  = "5.最低"
MEDIUM_LOW_STR              = "4.低"
MEDIUM_STR                  = "3.中"
MEDIUM_HIGH_STR             = "2.高"
HIGHEST_STR                 = "1.最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Simplified Chinese
;*******************************************************************************************
[Strings.0804]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "无线装置 开/关"
Disable                     = "停用"
Enable                      = "启用"
CountryRegion24G            = "频道代码 (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "频道代码 (5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒体/游戏环境"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "网络实体地址"
PSMode                      = "省电模式"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "随意网络支持802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

FAST_ROAMING_SENSITIVITY_STR = "漫游灵敏度" 
DISABLE_STR                 = "6.停用"
LOWEST_STR                  = "5.最低"
MEDIUM_LOW_STR              = "4.低"
MEDIUM_STR                  = "3.中"
MEDIUM_HIGH_STR             = "2.高"
HIGHEST_STR                 = "1.最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Japanese
;*******************************************************************************************
[Strings.0411]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "無線デバイス オン/オフ"
Disable                     = "無効"
Enable                      = "有効"
CountryRegion24G            = "チャンネルコード (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "チャンネルコード (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "マルチメディア/ゲーミング環境"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "ローカル管理されるMACアドレス"
PSMode                      = "省電力モード"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "11nのAdhocモード"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "ローミング感度"
DISABLE_STR                 = "6.無効"
LOWEST_STR                  = "5.最低"
MEDIUM_LOW_STR              = "4.低"
MEDIUM_STR                  = "3.中"
MEDIUM_HIGH_STR             = "2.高"
HIGHEST_STR                 = "1.最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Korean
;*******************************************************************************************
[Strings.0412]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "라디오 ON/OFF"
Disable                     = "사용 안함"
Enable                      = "사용함"
CountryRegion24G            = "국가/지역 (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "국가/지역 (5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "멀티미디어/게임 환경"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "로컬 관리 MAC 네트워크 주소"
PSMode                      = "절전 모드"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc 지원 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "로밍의 주동성" 
DISABLE_STR                 = "6.사용 안함"
LOWEST_STR                  = "5.최하"
MEDIUM_LOW_STR              = "4.낮음"
MEDIUM_STR                  = "3.보통"
MEDIUM_HIGH_STR             = "2.높음"
HIGHEST_STR                 = "1.최고" 

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- French
;*******************************************************************************************
[Strings.040c]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio Marche/Arrêt"
Disable                     = "Désactivé"
Enable                      = "Activé"
CountryRegion24G            = "Pays / Région (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Pays / Région (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Environnements Multimédia/Jeux"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Adresse Réseau d'Administration Locale MAC"
PSMode                      = "Mode Économie d'Énergie"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc Compatible 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensibilité" 
DISABLE_STR                 = "6.Désactivé"
LOWEST_STR                  = "5.le plus bas"
MEDIUM_LOW_STR              = "4.Basse"
MEDIUM_STR                  = "3.Intermédiaire"
MEDIUM_HIGH_STR             = "2.Haut"
HIGHEST_STR                 = "1.Le plus haut"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Italian
;*******************************************************************************************
[Strings.0410]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio Acceso/Spento"
Disable                     = "Disattiva"
Enable                      = "Attiva"
CountryRegion24G            = "Paese (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Paese (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente multimediale/giochi"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Indirizzo locale rete MAC"
PSMode                      = "Modalità risparmio energetico"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Modalità supporto 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensibilità" 
DISABLE_STR                 = "6.Disattiva"
LOWEST_STR                  = "5.più bassi"
MEDIUM_LOW_STR              = "4.Bassa"
MEDIUM_STR                  = "3.Medio"
MEDIUM_HIGH_STR             = "2.Alta"
HIGHEST_STR                 = "1.Più Alto"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- German
;*******************************************************************************************
[Strings.0407]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio An/Aus"
Disable                     = "Deaktivieren"
Enable                      = "Aktivieren"
CountryRegion24G            = "Land Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spielumgebung"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Lokale MAC Netzwerkadresse"
PSMode                      = "Stromsparmodus"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc Unterstützung 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Roaming-Empfindlichkeit" 
DISABLE_STR                 = "6.Deaktivieren"
LOWEST_STR                  = "5.Niedrigster"
MEDIUM_LOW_STR              = "4.Gering"
MEDIUM_STR                  = "3.Medium"
MEDIUM_HIGH_STR             = "2.Hoch"
HIGHEST_STR                 = "1.Höchsten"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Spanish
;*******************************************************************************************
[Strings.0c0a]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio Encendido/Apagado"
Disable                     = "Desactivar"
Enable                      = "Activar"
CountryRegion24G            = "Región País (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Región País (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Juego"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Dirección de Red MAC Local"
PSMode                      = "Modo Ahorrador de Energía"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "802.11n de soporte Adhoc"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Itinerancia de sensibilidad" 
DISABLE_STR                 = "6.Desactivar"
LOWEST_STR                  = "5.Más bajo"
MEDIUM_LOW_STR              = "4.Baja"
MEDIUM_STR                  = "3.Medio"
MEDIUM_HIGH_STR             = "2.Alto"
HIGHEST_STR                 = "1.Más alto"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Brazilian Portuguese
;*******************************************************************************************
[Strings.0416]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Rádio Ligado/Desligado"
Disable                     = "Desativar"
Enable                      = "Ativar"
CountryRegion24G            = "País Região (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "País Região (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Jogo"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Endereço de Rede MAC Local"
PSMode                      = "Modo Economizador de Energia"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "802.11n de suporte Adhoc"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Roaming Sensibilidade" 
DISABLE_STR                 = "6.Desativar"
LOWEST_STR                  = "5.Menor"
MEDIUM_LOW_STR              = "4.Baixa"
MEDIUM_STR                  = "3.Medium"
MEDIUM_HIGH_STR             = "2.Alta"
HIGHEST_STR                 = "1.Maior"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Dutch
;*******************************************************************************************
[Strings.0413]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Radio Aan/Uit"
Disable                     = "Uitschakelen"
Enable                      = "Inschakelen"
CountryRegion24G            = "Land regio (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land regio (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spelomgeving"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Lokaal MAC netwerkadres"
PSMode                      = "Stroombesparende modus"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc ondersteuning 802.11n"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Roaming Gevoeligheid"
DISABLE_STR                 = "6.Uitschakelen"
LOWEST_STR                  = "5.Laagste"
MEDIUM_LOW_STR              = "4.Laag"
MEDIUM_STR                  = "3.Medium"
MEDIUM_HIGH_STR             = "2.High"
HIGHEST_STR                 = "1.Hoogste"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

;*******************************************************************************************
; Strings --- Russian
;*******************************************************************************************
[Strings.0419]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter(rev.A2)"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"
D-Link_3C0F.DeviceDesc      = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
D-Link_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"
D-Link_3C16.DeviceDesc      = "D-Link DWA-125 Wireless N 150 USB Adapter(rev.A2)"
D-Link_3C17.DeviceDesc      = "D-Link DWA-121 Wireless N 150 USB Adapter"
D-Link_3C20.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.D)"
D-Link_3C21.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.C) "
D-Link_3C22.DeviceDesc      = "D-Link DWA-132 Wireless N USB Adapter(rev.B)"
D-Link_3C23.DeviceDesc      = "D-Link GO-USB-N300 Wireless N Easy USB Adapter"
D-Link_3C24.DeviceDesc      = "D-Link DWA-152 Wireless N Dual Band USB Adapter"
D-Link_3317.DeviceDesc      = "D-Link DWA-137 Wireless N High-Gain USB Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "Ralink 802.11n USB Wireless LAN Card Driver"
CTV1W.Service.DispName      = "Cisco CTV1W Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"

RadioOnOff                  = "Радио Вкл/Выкл"
Disable                     = "Выключить"
Enable                      = "Включить"
CountryRegion24G            = "Страна/регион (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Страна/регион (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Мультимедийная/Игровая среда"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Локальный MAC-адрес"
PSMode                      = "Режим энергосбережения"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Режим 802.11n прямого соединения"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"
FAST_ROAMING_SENSITIVITY_STR = "Роуминг Чувствительность" 
DISABLE_STR                 = "6.Выключить"
LOWEST_STR                  = "5.Самые низкие"
MEDIUM_LOW_STR              = "4.Низкий"
MEDIUM_STR                  = "3.Средний"
MEDIUM_HIGH_STR             = "2.Высокий"
HIGHEST_STR                 = "1.Высшая"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"
