;****************************************************************************************
;
; Drt2870.inf
;
;   This installation script supports Windows 2000 & XP for the
;   D-Link DWA series USB Wireless LAN Card.
;
;   Copyright (c)2002-2009 , D-Link Corp., All Rights Reserved
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %D-Link%
Compatible      = 1
DriverVer       = 04/15/2009, 1.04.03.0000
CatalogFile     = Drt2870.cat            ;for WHQL certified

[ControlFlags]
;***********D-Link 802.11 n board  ***********

[Manufacturer]
%D-Link%        = D-Link, NTamd64


[D-Link.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link_3C09.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C09
%D-Link_3C11.DeviceDesc%    = RTWLANH.ndi,          USB\VID_07D1&PID_3C11
%D-Link_3C13.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C13
%D-Link_3C0A.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C0A
%D-Link_3C0B.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C0B
%D-Link_3C0D.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C0D
%D-Link_3C0E.DeviceDesc%    = RTWLANSB.ndi,         USB\VID_07D1&PID_3C0E


;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RTWLANSB.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAN.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANR.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLAND.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANRG.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANH.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg ,CoInstOpt_DLink.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANHC.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg, CarrierDetect.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

[RTWLANS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, SmartScan.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles

; NT services sections
[RTWLANSB.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAN.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANR.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLAND.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANRG.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANH.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANHC.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

[RTWLANS.ndi.NT.Services]
AddService              = rt2870, 2, Generic.Service, common.EventLog

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************
[RTWLANSB.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAN.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANR.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLAND.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANRG.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANH.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANHC.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[RTWLANS.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable patch for pass wifi 11n draft
;
HKR, ,                            TGnWifiTest,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,       0, "0"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,              0, "1"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"

;
; RDG
;
HKR, ,                            RDG,      0, "1"

;
; Power Saving Control
;
HKR, ,                            PSControl,       0x00010001, 0x00000000

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,      0, "1"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,              ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan,              type,      0, "enum"
HKR, NDI\params\SmartScan,              default,   0, "0"
HKR, NDI\params\SmartScan\enum,         0,         0, %Disable%
HKR, NDI\params\SmartScan\enum,         1,         0, %Enable%

;
; AllowBW40InBGBand
;
HKR, ,                            AllowBW40InBGBand,      0, "1"

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, %PSPXlink%
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, %Disable%
HKR, NDI\params\PSPXlink\enum,    1,               0, %Enable%

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x0b034020"
HKR, Default,                     BACapability,      0x10001, "0x0b034020"


;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2ba15"


;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, %LocalNetworkAddress%
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""
HKR, NDI\params\Networkaddress,   optional,        0, "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, %PSMode%
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, %CAM%
HKR, NDI\params\PSMode\enum,      1,               0, %MAXPSP%

;
; CAM when AC Power
;
HKR, ,                            ACPowerCam,      0, "0"
HKR, Default,                     ACPowerCam,      0, "0"

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

;
; Reposit Bssid List
;
HKR, ,                BssidRepositTime,       0, "120"

[RemoveFlag.reg]
HKR, ,                SafelyRemoveOff,    0, "1"

[IEEE80211H.reg]
HKR, ,                IEEE80211H,         0, "1"

[CarrierDetect.reg]
HKR, ,                CarrierDetect,      0, "1"

[SmartScan.reg]
HKR, ,                SmartScan,          0, "1"

[AdhocN.reg]
;
; AdhocNMode
;
HKR, ,                            AdhocNMode,      0, "0"
HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
HKR, NDI\params\AdhocNMode,       type,            0, "enum"
HKR, NDI\params\AdhocNMode,       default,         0, "0"
HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable%

; Disable Channel 14 for JP
[InitChn14Disabled.reg]
HKR, ,                    InitChn14Disabled,      0,"1"

[SingleBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

[DefaultBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; 5G Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%
HKR, NDI\params\CountryRegionABand\enum,11,                0, %CountryRegion5G_11%
HKR, NDI\params\CountryRegionABand\enum,12,                0, %CountryRegion5G_12%
HKR, NDI\params\CountryRegionABand\enum,13,                0, %CountryRegion5G_13%
HKR, NDI\params\CountryRegionABand\enum,14,                0, %CountryRegion5G_14%
HKR, NDI\params\CountryRegionABand\enum,15,                0, %CountryRegion5G_15%
HKR, NDI\params\CountryRegionABand\enum,16,                0, %CountryRegion5G_16%

;
; RaCoInstaller Options
; CoInstaller Options , Enable 11n feature in Morocco, Russia, Ukraine.
[CoInstOpt_DLink.reg]
HKR, ,                            RaCoInstOpt,      0,"00001111"
; WirelessMode
HKR, ,                            WirelessMode,    0, "5"
; CountryWirelessMode
HKR, ,                            CountryWirelessMode,    0x10001, "0x11101110"

; CoInstaller Options for Azurewave
[CoInstOpt_Az.reg]
HKR, ,                    RaCoInstOpt,      0,"00001111"

; WirelessMode
HKR, ,                            WirelessMode,    0, "3"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInstx.dll,ClassCoInstaller"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
CoInstaller.CopyFiles   = 11

[NT.CopyFiles]
rt2870.sys                       ; NT Installation

[CoInstaller.CopyFiles]
RaCoInstx.dll
RaCoInst.dat

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt2870.sys              = 1
RaCoInstx.dll           = 1
RaCoInst.dat            = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "rt2870"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\rt2870.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2870.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
D-Link                      = "D-Link Corporation"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
D-Link_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
D-Link_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
D-Link_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter"
D-Link_3C0E.DeviceDesc      = "D-Link WUA-2340 USB Adapter(rev.B)"


INSTALL_DISK_STR            = "D-Link Wireless 11n USB Installation Disk"
Generic.Service.DispName    = "D-Link 802.11n USB Wireless LAN Card Driver"

;
; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
; SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11 Wireless Card."
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "D-Link Client"

RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
PSPXlink                    = "PSP Xlink Mode"
LocalNetworkAddress         = "Local MAC Network Address"
PSMode                      = "Power Saving Mode"
CAM                         = "CAM"
MAXPSP                      = "Max_PSP"
AdhocNMode                  = "Adhoc support 802.11n"

