DNS-1100-04 Compatibility List 2012-08-14

Compatible HDD List

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Vendor  | Family  | Model  | Interface  | Capacity  | Sector Format | Firmware  |
| Hitachi  | Deskstar 7K1000 | HDT721010KLA330 | SATA3G HDD  | 1TB | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K1000.B | HDT721010SLA360 | SATA3G HDD  | 1TB | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K1000.C | HDS721050CLA362 | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K160  | HDS721680PLA380  | SATA 3G HDD  | 80G  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K160  | HDS721680PLA380  | SATA 3G HDD  | 82G  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K2000 | HDS722020ALA330 | SATA 3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar 7K3000 | HDS723030ALA640 | SATA 6G HDD  | 3TB  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar P7K500  | HDP725050GLA360  | SATA 3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar T7K500  | HDT725032VLA360  | SATA 3G HDD  | 320G  | 512 bytes | 1.00b11 |
| Hitachi  | Deskstar7K1000  | HDS721010KLA330  | SATA 3G HDD  | 1TB  | 512 bytes | 1.00b11 |
| Hitachi | Deskstar 5K1000 | HDS5C1010CLA382 | SATA3G HDD  | 1TB  | 512 bytes | 1.01b01 |
| Hitachi | Deskstar 5K3000 | HDS5C3020ALA632 | SATA6G HDD  | 2TB  | 512 bytes | 1.01b01 |
| Hitachi  | CinemaStar 5K2000 | HCS5C2020ALA632 | SATA6G HDD  | 2TB  | 4K bytes | 1.01b01 |
| Hitachi  | Deskstar 7K3000 | HDS723020BLA642 | SATA6G HDD  | 2TB  | 512 bytes | 1.01b01 |
| Hitachi  | Deskstar 7k1000.D | HDS721010DLE630 | SATA6G HDD  | 1TB  | 512 bytes | 1.01b08 |
| Maxtor  | DiamondMax 20  | STM3160811AS  | SATA 3G HDD  | 160G  | 512 bytes | 1.00b11 |
| Maxtor  | DiamondMax 21  | STM3500320AS  | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Maxtor  | DiamondMax 22  | STM3750330AS  | SATA3G HDD  | 750G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.10  | ST3320620AS  | SATA 3G HDD  | 320G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.10  | ST3320820AS  | SATA 3G HDD  | 320G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.11  | ST3640323AS  | SATA 3G HDD  | 640G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.11  | ST31000333AS  | SATA 3G HDD  | 1TB  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.12  | ST31000528AS  | SATA3G HDD  | 1TB  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda 7200.12  | ST3500418AS  | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda ES  | ST3750640NS  | SATA3G HDD  | 750G  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda LP | ST3200542AS | SATA3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda XT | ST32000641AS | SATA3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda XT | ST33000651AS | SATA6G HDD  | 3TB  | 512 bytes | 1.00b11 |
| Seagate  | Barracuda® Green  | ST2000DL003  | SATA6G HDD  | 2TB  | 4K bytes | 1.00b11 |
| Seagate  | Constellation™ ES | ST32000644NS | SATA3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Seagate  | SV 35.3  | ST31000340SV  | SATA3G HDD  | 1TB  | 512 bytes | 1.00b11 |
| Seagate  | SV35.4  | ST3320410SV  | SATA3G HDD  | 320G  | 512 bytes | 1.00b11 |
| Seagate | Barracuda 7200.12 | ST31000524AS | SATA6G HDD  | 1TB  | 512 bytes | 1.01b01 |
| Seagate | Barracuda LP | ST1500DL003 | SATA6G HDD  | 1.5TB  | 4K bytes | 1.01b01 |
| Seagate | Constellation™ ES | ST33000650NS | SATA6G HDD  | 3TB | 512 bytes | 1.01b01 |
| Seagate | Barracuda  | ST1000DM003 | SATA6G HDD  | 1TB  | 512 Bytes | 1.01b08 |
| Seagate | Barracuda  | ST2000DM001 | SATA6G HDD  | 2TB  | 512 Bytes | 1.01b08 |
| Seagate  | Barracuda® 7200.12 | ST3000DM001 | SATA6G HDD  | 3TB | 512 bytes | 1.01b08 |
| Western Digital  | AV series  | WD5000AVJS  | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Western Digital  | Caviar Black  | WD5001AALS  | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Western Digital  | Caviar Black  | WD6402AAEX | SATA6G HDD  | 640G  | 512 bytes | 1.00b11 |
| Western Digital  | Caviar Black  | WD7501AALS  | SATA3G HDD  | 750G  | 512 bytes | 1.00b11 |
| Western Digital  | Caviar Black  | WD2002FAEX | SATA6G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Western Digital  | Caviar Blue | WD10EALS | SATA 3G HDD  | 1TB | 512 bytes | 1.00b11 |
| Western Digital  | VelociRaptor  | WD3000HLFS  | SATA3G HDD  | 300G  | 512 bytes | 1.00b11 |
| Western Digital  | VelociRaptor  | WD6000HLHX | SATA 6G HDD  | 600G  | 512 bytes | 1.00b11 |
| Western Digital  | WD Caviar ®Green  | WD20EADS  | SATA3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Western Digital  | WD Caviar ®Green  | WD6400AARS | SATA3G HDD  | 640G  | 4K bytes | 1.00b11 |
| Western Digital  | WD Caviar ®Green  | WD20EARS  | SATA6G HDD  | 2TB  | 4K bytes | 1.00b11 |
| Western Digital  | WD Caviar ®Green  | WD30EZRX | SATA6G HDD  | 3TB  | 4K bytes | 1.00b11 |
| Western Digital  | WD Caviar GP  | WD5000AACS  | SATA3G HDD  | 500G  | 512 bytes | 1.00b11 |
| Western Digital  | WD Caviar SE16  | WD7500AAKS  | SATA 3G HDD  | 750G  | 512 bytes | 1.00b11 |
| Western Digital  | WD Caviar SE16  | WD2500AAKS  | SATA 3G HDD  | 250G | 512 bytes | 1.00b11 |
| Western Digital  | WD Raptor  | WD1500ADFD  | SATA 3G HDD  | 150G  | 512 bytes | 1.00b11 |
| Western Digital  | WD RE  | WD1600YS  | SATA3G HDD  | 160G  | 512 bytes | 1.00b11 |
| Western Digital  | WD RE2  | WD7500AYYS  | SATA3G HDD  | 750G  | 512 bytes | 1.00b11 |
| Western Digital  | WD RE4 -GP | WD2002FYPS | SATA3G HDD  | 2TB  | 512 bytes | 1.00b11 |
| Western Digital  | WD Red | WD10EFRX | SATA6G HDD  | 1TB | 512 bytes | 1.01b08 |
| Western Digital  | WD Red | WD20EARX | SATA6G HDD  | 2TB | 4K bytes | 1.01b08 |
| Western Digital  | WD Red | WD30EFRX | SATA6G HDD  | 3TB | 512 bytes | 1.01b08 |

Compatible Printer List

|  |  |  |  |
| --- | --- | --- | --- |
| **Brand** | **Model**  | **OS** | **Printer Driver Version** |
| Brother | DCP-7030 | Windows XP | B2 |
| Windows Vista | B2 |
| Windows 7 | A2 |
| Epson  | TX320F | Windows XP | 6.71  |
| Windows Vista | 6.71  |
| Windows 7 | 6.71  |
| HP | Deskjet F380 | Windows XP | 7.0.2 |
| Windows Vista | 080.001.237.001 |
| Windows 7 | 13.1.0 |
| HP | Deskjet F4185 | Windows XP | 9.0.1 |
| Windows Vista | 9.0.1 |
| Windows 7 | 13.1.0 |
| Canon | PIXMA MP180 | Windows XP | 1.11 |
| Windows Vista | 1.11 |
| Windows 7 | 1.11 |
| Canon | PIXMA MP160 | Windows XP | 1.11 |
| Windows Vista | 1.11 |
| Windows 7 | 1.11 |
| Epson | STYLUS CX5700F | Windows XP | 5.50 |
| Windows Vista | 6.5aE |
| Windows 7 | 6.52 |
| Samsung | SCX-4200 | Windows XP | 3.04.96:05 |
| Windows Vista | 3.04.96:05 |
| Windows 7 | 3.04.96:05 |
| HP | Officejet 4355 | Windows XP | 60.53.243.0 |
| Windows Vista | 61.53.25.9 |
| Windows 7 | 61.53.25.9 |
| Brother | MFC-J410 | Windows XP | B2 |
| Windows Vista | B2 |
| Windows 7 | A2 |
| HP | Officejet 4255 | Windows XP | 4.7.1 |
| Windows Vista | 61.53.25.9 |
| Windows 7 | 61.53.25.9 |
| HP | Laserjet 3050 | Windows XP | 60.63.461.42 |
| Windows Vista | 60.63.461.42 |
| Windows 7 | 60.63.461.42 |
| Epson | AcuLaser MX14 | Windows XP | 1.1 |
| Windows Vista | 1.1 |
| Windows 7 | 1.1 |
| Samsung | SCX-4623F | Windows XP | 3.10.49:14 |
| Windows Vista | 3.10.49:14 |
| Windows 7 | 3.10.49:14 |
| Epson | Stylus Photo RX590 | Windows XP | 6.11E |
| Windows Vista | 6.11E |
| Windows 7 | 6.11E |
| HP | Officejet J4580 | Windows XP | 10.0.0 |
| Windows Vista | 10.0.0 |
| Windows 7 | 13.0.0 |

2012/08/14