;****************************************************************************************
;
; netr28ux.inf
;
;   This installation script supports Windows Vista for the
;   Ralink RT2870 series USB Wireless LAN Card.
;
;   Copyright (c)2008 , Ralink Technology Corp., All Rights Reserved
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;**************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
Compatible      = 1
CatalogFile     = netr28ux.cat ; For WHQL certification.
DriverVer       = 08/21/2008, 2.02.02.0000

[ControlFlags]
;***********Ralink 802.11n board  ***********
;ExcludeFromSelect = USB\VID_148F&PID_2870

[Manufacturer]
%Ralink%        = Ralink, NTamd64
%Asus%          = ASUS, NTamd64
%Sitecom%       = Sitecom, NTamd64
%Conceptronic%  = Conceptronic, NTamd64
%Planex%        = Planex, NTamd64
%D-Link%        = D-Link, NTamd64
%AL%            = AL, NTamd64
%Airlink%       = Airlink, NTamd64
%Corega%        = Corega, NTamd64
%Corega_TW%     = Corega_TW, NTamd64
%Gigabyte%      = Gigabyte, NTamd64
%Sparklan%      = Sparklan, NTamd64
%SMC%           = SMC, NTamd64
%Arcadyan%      = Arcadyan, NTamd64
%ZCOM%          = ZCOM, NTamd64
%ZyXEL%         = ZyXEL, NTamd64
%EnGenius%      = EnGenius, NTamd64
%Philips%       = Philips, NTamd64
%Draytek%       = Draytek, NTamd64
%AzureWave%     = AzureWave, NTamd64
%Accton%        = Accton, NTamd64
%AMIT%          = AMIT, NTamd64
%Hawking%       = Hawking, NTamd64
%Siemens%       = Siemens, NTamd64
%Edimax%        = Edimax, NTamd64
%AboCom%        = AboCom, NTamd64
%BUFFALO%       = BUFFALO, NTamd64
%Gemtek%        = Gemtek, NTamd64
%Amigo%         = Amigo, NTamd64
%PEGATRON%      = PEGATRON, NTamd64
%LevelOne%      = LevelOne, NTamd64
%Quanta%        = Quanta, NTamd64
%Zinwell%       = Zinwell, NTamd64
%Logitec%       = Logitec, NTamd64

[Ralink.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Generic.DeviceDesc%        = Ralink.ndi,           USB\VID_148F&PID_2870
%Generic.DeviceDesc%        = Ralink_2770.ndi,      USB\VID_148F&PID_2770
%GenericWLAN.DeviceDesc%    = Ralink_2070.ndi,      USB\VID_148F&PID_2070
%GenericWLAN.DeviceDesc%    = Ralink_3070.ndi,      USB\VID_148F&PID_3070
; Qcom
%Generic.DeviceDesc%        = Qcom_2770.ndi,        USB\VID_18E8&PID_6259

[ASUS.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS_1731.DeviceDesc%      = ASUS.ndi,             USB\VID_0B05&PID_1731
%ASUS_1732.DeviceDesc%      = ASUS.ndi,             USB\VID_0B05&PID_1732
%ASUS_1742.DeviceDesc%      = ASUS_RemoveFlag.ndi,  USB\VID_0B05&PID_1742
%ASUS_1760.DeviceDesc%      = ASUS_RemoveFlag.ndi,  USB\VID_0B05&PID_1760
%ASUS_1761.DeviceDesc%      = ASUS.ndi,             USB\VID_0B05&PID_1761

[Sitecom.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom_0017.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_0017
%Sitecom_002B.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_002B
%Sitecom_002C.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_002C
%Sitecom_002D.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_002D
%Sitecom_0039.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_0039
%Sitecom_003B.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_003B
%Sitecom_003C.DeviceDesc%   = Sitecom.ndi,          USB\VID_0DF6&PID_003C

[Conceptronic.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic_3C06.DeviceDesc%   = Conceptronic.ndi,     USB\VID_14B2&PID_3C06
%Conceptronic_3C28.DeviceDesc%   = Conceptronic.ndi,     USB\VID_14B2&PID_3C28

[Planex.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Planex_ED06.DeviceDesc%    = Planex.ndi,           USB\VID_2019&PID_ED06
%Planex_AB25.DeviceDesc%    = Planex.ndi,           USB\VID_2019&PID_AB25

[D-Link.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%D-Link_3C09.DeviceDesc%    = D-Link.ndi,           USB\VID_07D1&PID_3C09
%D-Link_3C11.DeviceDesc%    = D-Link_3C11.ndi,      USB\VID_07D1&PID_3C11
%D-Link_3C13.DeviceDesc%    = D-Link.ndi,           USB\VID_07D1&PID_3C13

[AL.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AL_3C07.DeviceDesc%        = AL.ndi,               USB\VID_14B2&PID_3C07
%AL_3C12.DeviceDesc%        = AL.ndi,               USB\VID_14B2&PID_3C12

[Airlink.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Airlink_3C23.DeviceDesc%   = Airlink.ndi,          USB\VID_14B2&PID_3C23
%Airlink_3C27.DeviceDesc%   = Airlink.ndi,          USB\VID_14B2&PID_3C27

[Corega.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega_002F.DeviceDesc%    = Corega.ndi,           USB\VID_07AA&PID_002F
%Corega_003C.DeviceDesc%    = Corega.ndi,           USB\VID_07AA&PID_003C
%Corega_003F.DeviceDesc%    = Corega_003F.ndi,      USB\VID_07AA&PID_003F

[Corega_TW.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega_TW_0012.DeviceDesc% = Corega_TW.ndi,        USB\VID_18C5&PID_0012

[Gigabyte.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gigabyte_800B.DeviceDesc%  = Gigabyte.ndi,         USB\VID_1044&PID_800B
%Gigabyte_800C.DeviceDesc%  = Gigabyte.ndi,         USB\VID_1044&PID_800C
%Gigabyte_800D.DeviceDesc%  = Gigabyte.ndi,         USB\VID_1044&PID_800D

[Sparklan.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sparklan.DeviceDesc%       = Sparklan.ndi,         USB\VID_15A9&PID_0006

[SMC.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SMC_B522.DeviceDesc%       = SMC.ndi,              USB\VID_083A&PID_B522
%SMC_A618.DeviceDesc%       = SMC.ndi,              USB\VID_083A&PID_A618

[Arcadyan.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Arcadyan_7522.DeviceDesc%  = Arcadyan.ndi,         USB\VID_083A&PID_7522
%Arcadyan_8522.DeviceDesc%  = Arcadyan.ndi,         USB\VID_083A&PID_8522
%Arcadyan_7512.DeviceDesc%  = Arcadyan.ndi,         USB\VID_083A&PID_7512
%Arcadyan_7511.DeviceDesc%  = Arcadyan.ndi,         USB\VID_083A&PID_7511

[ZCOM.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZCOM.DeviceDesc%           = ZCOM.ndi,             USB\VID_0CDE&PID_0022

[ZyXEL.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZyXEL_3416.DeviceDesc%     = ZyXEL.ndi,            USB\VID_0586&PID_3416
%ZyXEL_0025.DeviceDesc%     = ZyXEL.ndi,            USB\VID_0CDE&PID_0025

[EnGenius.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%EnGenius_9701.DeviceDesc%  = EnGenius.ndi,         USB\VID_1740&PID_9701
%EnGenius_9702.DeviceDesc%  = EnGenius.ndi,         USB\VID_1740&PID_9702
%EnGenius_9703.DeviceDesc%  = EnGenius.ndi,         USB\VID_1740&PID_9703

[Philips.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Philips.DeviceDesc%        = Philips.ndi,          USB\VID_0471&PID_200F

[Draytek.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Draytek.DeviceDesc%        = Draytek.ndi,          USB\VID_14B2&PID_3C25

[AzureWave.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AzureWave_3247.DeviceDesc% = AzureWave_RemoveFlag.ndi,        USB\VID_13D3&PID_3247
%AzureWave_3262.DeviceDesc% = AzureWave_RemoveFlag.ndi,        USB\VID_13D3&PID_3262
%AzureWave_3273.DeviceDesc% = AzureWave_RemoveFlag.ndi,        USB\VID_13D3&PID_3273

[Accton.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Accton.DeviceDesc%         = Accton.ndi,           USB\VID_083A&PID_6618

[AMIT.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT.ndi,             USB\VID_18C5&PID_0008

[Hawking.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Hawking_0001.DeviceDesc%   = Hawking.ndi,          USB\VID_0E66&PID_0001
%Hawking_0003.DeviceDesc%   = Hawking.ndi,          USB\VID_0E66&PID_0003
%Hawking_0009.DeviceDesc%   = Hawking.ndi,          USB\VID_0E66&PID_0009
%Hawking_000B.DeviceDesc%   = Hawking.ndi,          USB\VID_0E66&PID_000B

[Siemens.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Siemens.DeviceDesc%        = Siemens.ndi,          USB\VID_129B&PID_1828

[Edimax.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Edimax_7717.DeviceDesc%    = Edimax.ndi,           USB\VID_7392&PID_7717
%Edimax_7718.DeviceDesc%    = Edimax.ndi,           USB\VID_7392&PID_7718
%Edimax_7711.DeviceDesc%    = Edimax.ndi,           USB\VID_7392&PID_7711

[AboCom.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AboCom_2770.DeviceDesc%    = AboCom.ndi,           USB\VID_07B8&PID_2770
%AboCom_2870.DeviceDesc%    = AboCom.ndi,           USB\VID_07B8&PID_2870
%AboCom_AB24.DeviceDesc%    = AboCom.ndi,           USB\VID_2019&PID_AB24
%AboCom_3070.DeviceDesc%    = AboCom.ndi,           USB\VID_07B8&PID_3070
%AboCom_3071.DeviceDesc%    = AboCom.ndi,           USB\VID_07B8&PID_3071

[BUFFALO.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%BUFFALO_012E.DeviceDesc%   = BUFFALO.ndi,          USB\VID_0411&PID_012E

[Gemtek.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Gemtek_0010.DeviceDesc%    = Gemtek.ndi,           USB\VID_15A9&PID_0010

[Amigo.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Amigo_9031.DeviceDesc%     = Amigo.ndi,            USB\VID_0E0B&PID_9031
%Amigo_9041.DeviceDesc%     = Amigo.ndi,            USB\VID_0E0B&PID_9041

[PEGATRON.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%PEGATRON_0001.DeviceDesc%  = PEGATRON.ndi,         USB\VID_1D4D&PID_0001
%PEGATRON_0002.DeviceDesc%  = PEGATRON.ndi,         USB\VID_1D4D&PID_0002

[LevelOne.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%LevelOne_0605.DeviceDesc%  = LevelOne.ndi,         USB\VID_1740&PID_0605
%LevelOne_0615.DeviceDesc%  = LevelOne.ndi,         USB\VID_1740&PID_0615

[Quanta.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Quanta_0304.DeviceDesc%    = Quanta.ndi,           USB\VID_1A32&PID_0304

[Zinwell.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Zinwell_0280.DeviceDesc%   = Zinwell.ndi,          USB\VID_5A57&PID_0280
%Zinwell_0282.DeviceDesc%   = Zinwell.ndi,          USB\VID_5A57&PID_0282

[Logitec.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Logitec_0162.DeviceDesc%   = Logitec.ndi,          USB\VID_0789&PID_0162
%Logitec_0163.DeviceDesc%   = Logitec.ndi,          USB\VID_0789&PID_0163
%Logitec_0164.DeviceDesc%   = Logitec.ndi,          USB\VID_0789&PID_0164

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[Ralink.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Ralink_2770.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Ralink_2070.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Ralink_3070.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Qcom_2770.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[ASUS.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[ASUS_RemoveFlag.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Sitecom.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Conceptronic.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Planex.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[D-Link.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[D-Link_3C11.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, IEEE80211H.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[AL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Airlink.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Corega.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Corega_003F.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, IEEE80211H.reg, CarrierDetect.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Corega_TW.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Gigabyte.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Sparklan.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[SMC.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Arcadyan.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[ZCOM.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[ZyXEL.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[EnGenius.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Philips.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Draytek.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[AzureWave_RemoveFlag.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Accton.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[AMIT.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Hawking.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Siemens.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Edimax.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[AboCom.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[BUFFALO.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Gemtek.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg, SmartScan.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Amigo.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[PEGATRON.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[LevelOne.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Quanta.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Zinwell.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[Logitec.ndi.NT]
AddReg                  = Common.reg, RTUSB.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

; NT services sections
[Ralink.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Ralink_2770.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Ralink_2070.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Ralink_3070.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Qcom_2770.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[ASUS.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[ASUS_RemoveFlag.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Sitecom.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Conceptronic.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Planex.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[D-Link.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[D-Link_3C11.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[AL.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Airlink.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Corega.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Corega_003F.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Corega_TW.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Gigabyte.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Sparklan.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Arcadyan.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[ZCOM.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[ZyXEL.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[EnGenius.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Philips.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Draytek.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[AzureWave_RemoveFlag.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Accton.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[AMIT.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Hawking.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Siemens.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Edimax.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[AboCom.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[BUFFALO.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Gemtek.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Amigo.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[PEGATRON.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[LevelOne.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Quanta.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Zinwell.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[Logitec.ndi.NT.Services]
AddService              = netr28ux, 2, Generic.Service, common.EventLog

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************
[Ralink.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Ralink_2770.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Ralink_2070.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Ralink_3070.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Qcom_2770.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[ASUS.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[ASUS_RemoveFlag.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Sitecom.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Conceptronic.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Planex.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[D-Link.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[D-Link_3C11.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[AL.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Airlink.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Corega.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Corega_003F.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Corega_TW.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Gigabyte.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Sparklan.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[SMC.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Arcadyan.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[ZCOM.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[ZyXEL.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[EnGenius.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Philips.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Draytek.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[AzureWave_RemoveFlag.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Accton.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[AMIT.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Hawking.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Siemens.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Edimax.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[AboCom.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[BUFFALO.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Gemtek.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Amigo.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[PEGATRON.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[LevelOne.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Quanta.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Zinwell.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[Logitec.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"
HKR, NDI\params\TXBurst,                ParamDesc, 0, %TXBurst%
HKR, NDI\params\TXBurst,                type,      0, "enum"
HKR, NDI\params\TXBurst,                default,   0, "1"
HKR, NDI\params\TXBurst\enum,           0,         0, %Disable%
HKR, NDI\params\TXBurst\enum,           1,         0, %Enable%

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%
HKR, NDI\params\CountryRegionABand\enum,11,                0, %CountryRegion5G_11%
HKR, NDI\params\CountryRegionABand\enum,12,                0, %CountryRegion5G_12%

;
; RDG
;
HKR, ,                            RDG,      0, "1"
HKR, NDI\params\RDG,                    ParamDesc, 0, %RDG%
HKR, NDI\params\RDG,                    type,      0, "enum"
HKR, NDI\params\RDG,                    default,   0, "1"
HKR, NDI\params\RDG\enum,               0,         0, %Disable%
HKR, NDI\params\RDG\enum,               1,         0, %Enable%

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, %WMMCapable%
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, %Disable%
HKR, NDI\params\WMMCapable\enum,        1,         0, %Enable%

;
; HTCapable
;
;HKR, ,                            HTCapable,      0, "1"
;HKR, NDI\params\HTCapable,             ParamDesc, 0, %HTCapable%
;HKR, NDI\params\HTCapable,             type,      0, "enum"
;HKR, NDI\params\HTCapable,             default,   0, "1"
;HKR, NDI\params\HTCapable\enum,        0,         0, %Disable%
;HKR, NDI\params\HTCapable\enum,        1,         0, %Enable%

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"
HKR, NDI\params\CarrierDetect,       ParamDesc,       0, %CarrierDetect%
HKR, NDI\params\CarrierDetect,       type,            0, "enum"
HKR, NDI\params\CarrierDetect,       default,         0, "0"
HKR, NDI\params\CarrierDetect\enum,  0,               0, %Disable%
HKR, NDI\params\CarrierDetect\enum,  1,               0, %Enable%

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,              ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan,              type,      0, "enum"
HKR, NDI\params\SmartScan,              default,   0, "0"
HKR, NDI\params\SmartScan\enum,         0,         0, %Disable%
HKR, NDI\params\SmartScan\enum,         1,         0, %Enable%

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x0b034040"
HKR, Default,                     BACapability,      0x10001, "0x0b034040"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2ba15"

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

[RemoveFlag.reg]
HKR, ,                SafelyRemoveOff,    0, "1"

[IEEE80211H.reg]
HKR, ,                IEEE80211H,         0, "1"

[CarrierDetect.reg]
HKR, ,                CarrierDetect,      0, "1"

[SmartScan.reg]
HKR, ,                SmartScan,          0, "1"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInstx.dll,ClassCoInstaller"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************
[NT.CopyFiles]
netr28ux.sys,,,2

[CoInstaller.CopyFiles]
RaCoInstx.dll,,,2
RaCoInst.dat,,,2

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
netr28ux.sys                = 1,,
RaCoInstx.dll               = 1,,
RaCoInst.dat                = 1,,

[DestinationDirs]
NT.CopyFiles     = 12     ; system32\drivers subdirectory on NT
DefaultDestDir   = 11
CoInstaller.CopyFiles	= 11

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "netr28ux"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "wlan, ethernet"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\netr28ux.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\netr28ux.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "Ralink"
Ralink                      = "Ralink Technology, Corp."
Asus                        = "ASUSTeK Computer Inc."
Sitecom                     = "Sitecom Europe BV"
Conceptronic                = "Conceptronic"
Planex                      = "Planex Communications, Inc."
D-Link                      = "D-Link"
AL                          = "AL Tech., Inc."
Airlink                     = "Airlink"
Corega                      = "corega"
Corega_TW                   = "corega Taiwan Inc."
Gigabyte                    = "Gigabyte Technology Corp."
Sparklan                    = "Sparklan Communications, Inc."
SMC                         = "SMC Networks, Inc."
Arcadyan                    = "Arcadyan Technology Corporation"
ZCOM                        = " "
ZyXEL                       = "ZyXEL Communications Corporation"
EnGenius                    = "EnGenius Technologies"
Philips                     = "Philips"
Draytek                     = "Draytek"
AzureWave                   = "AzureWave Technologies, Inc."
Accton                      = "Accton Technology Corp."
AMIT                        = "AMIT Technology, Inc."
Hawking                     = "Hawking Technologies"
Siemens                     = "Siemens"
Edimax                      = "Edimax Technology Co., Ltd"
AboCom                      = "AboCom System, Inc."
BUFFALO                     = "BUFFALO INC"
Gemtek                      = "Gemtek"
Amigo                       = "Amigo Technology Inc."
PEGATRON                    = "PEGATRON CORPORATION"
LevelOne                    = "LevelOne"
Quanta                      = "Quanta Microsystems, Inc."
Zinwell                     = "Zinwell Corporation"
Logitec                     = "Logitec Corporation"

GenericWLAN.DeviceDesc      = "802.11 USB Wireless LAN Card"
Generic.DeviceDesc          = "802.11n USB Wireless LAN Card"
ASUS_1731.DeviceDesc        = "ASUS 802.11n Network Adapter"
ASUS_1732.DeviceDesc        = "802.11n Network Adapter"
ASUS_1742.DeviceDesc        = "802.11n Network Adapter"
ASUS_1760.DeviceDesc        = "802.11n Network Adapter"
ASUS_1761.DeviceDesc        = "ASUS 802.11n Network Adapter"
Sitecom_0017.DeviceDesc     = "Sitecom Wireless-N Network USB Card WL-182"                       
Sitecom_002B.DeviceDesc     = "Sitecom Wireless Network 300N USB Adapter WL-188"
Sitecom_002C.DeviceDesc     = "Wireless Network 300N USB adapter WL-301"
Sitecom_002D.DeviceDesc     = "Wireless Network 300N USB dongle WL-302"
Sitecom_0039.DeviceDesc     = "Sitecom Wireless-N USB Adapter WL-315"
Sitecom_003B.DeviceDesc     = "Sitecom Intelligent Wireless Gaming Adapter WL-321"
Sitecom_003C.DeviceDesc     = "Sitecom Wireless-N USB Adapter WL-323"
Conceptronic_3C06.DeviceDesc= "Conceptronic 802.11n USB adapter (V1)"
Conceptronic_3C28.DeviceDesc= "Conceptronic 802.11n USB adapter (V2)"
Planex_ED06.DeviceDesc      = "PCI 802.11n Wireless LAN USB Adapter"
Planex_AB25.DeviceDesc      = "150N Wireless LAN USB Adapter"
D-Link_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
D-Link_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
D-Link_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
AL_3C07.DeviceDesc          = "AnyGate 11N W-LAN Adapter (XM-242U)"
AL_3C12.DeviceDesc          = "AnyGate 11n W-LAN Adapter (XM-200U)"
Airlink_3C23.DeviceDesc     = "Airlink101 300N Wireless USB Adapter"
Airlink_3C27.DeviceDesc     = "Airlink101 Wireless USB Adapter"
Corega_002F.DeviceDesc      = "CG-WLUSB2GNL"
Corega_003C.DeviceDesc      = "CG-WLUSB2GNL"
Corega_003F.DeviceDesc      = "CG-WLUSB300AGN"
Corega_TW_0012.DeviceDesc   = "CG-WLUSB10 corega Wireless USB Adapter"                               
Gigabyte_800B.DeviceDesc    = "Gigabyte GN-WB30N 802.11n USB WLAN Card"
Gigabyte_800C.DeviceDesc    = "Gigabyte GN-WB31N 802.11n USB WLAN Card"
Gigabyte_800D.DeviceDesc    = "Gigabyte GN-WB32L 802.11n USB WLAN Card"
Sparklan.DeviceDesc         = "Wireless 11n USB Adapter"
SMC_B522.DeviceDesc         = "EZ Connect N Draft 11n Wireless USB2.0 Adapter"
SMC_A618.DeviceDesc         = "SMC EZ Connect N Draft 11n Wireless USB 2.0 Adapter"
Arcadyan_7522.DeviceDesc    = "802.11N Wireless USB Adapter"
Arcadyan_8522.DeviceDesc    = "802.11N Wireless USB Adapter"
Arcadyan_7512.DeviceDesc    = "802.11N Wireless USB Adapter"
Arcadyan_7511.DeviceDesc    = "802.11N Wireless USB Adpater"
ZCOM.DeviceDesc             = "802.11b/g/n USB Wireless Network Adapter"
ZyXEL_3416.DeviceDesc       = "802.11n Wireless USB Adapter"
ZyXEL_0025.DeviceDesc       = "802.11b/g/n USB Wireless Network Adapter"
EnGenius_9701.DeviceDesc    = "EnGenius 802.11n Wireless USB Adapter"
EnGenius_9702.DeviceDesc    = "EnGenius 802.11n Wireless USB Adapter"
EnGenius_9703.DeviceDesc    = "EnGenius 802.11n Wireless USB Adapter"
Philips.DeviceDesc          = "Philips 802.11n Wireless USB Adapter"
Draytek.DeviceDesc          = "Vigor N61 802.11n Wireless USB Adapter"
AzureWave_3247.DeviceDesc   = "802.11 n/g/b Wireless LAN USB Adapter"
AzureWave_3262.DeviceDesc   = "802.11 n/g/b Wireless LAN USB Adapter"
AzureWave_3273.DeviceDesc   = "802.11 n/g/b Wireless LAN USB Mini-Card"
Accton.DeviceDesc           = "802.11n Wireless USB Adapter"
AMIT.DeviceDesc             = "CG-WLUSB2GNR, corega Wireless USB Adapter"
Hawking_0001.DeviceDesc     = "HWUN1 Hawking Technologies Hi-Gain Wireless-300N USB Adapter w/ Upgradable Antenna"
Hawking_0003.DeviceDesc     = "HWDN1 Hawking Technologies Hi-Gain USB Wireless-300N Dish Adapter"
Hawking_0009.DeviceDesc     = "HWUN2 Hawking Technologies Hi-Gain Wireless-150N USB Adapter w/ Upgradable Antenna"
Hawking_000B.DeviceDesc     = "HWDN2 Hawking Technologies Hi-Gain USB Wireless-150N Dish Adapter"
Siemens.DeviceDesc          = "Gigaset USB Adapter 300"
Edimax_7717.DeviceDesc      = "Edimax 802.11n Wireless USB Adapter"
Edimax_7718.DeviceDesc      = "Edimax 802.11n Wireless USB Adapter"
Edimax_7711.DeviceDesc      = "Edimax nLite Wireless USB Adapter"
AboCom_2770.DeviceDesc      = "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
AboCom_2870.DeviceDesc      = "802.11n/b/g Wireless LAN USB2.0 Adapter"
AboCom_AB24.DeviceDesc      = "GW-US300MiniS"
AboCom_3070.DeviceDesc      = "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
AboCom_3071.DeviceDesc      = "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
BUFFALO_012E.DeviceDesc     = "802.11n USB Wireless Card"
Gemtek_0010.DeviceDesc      = "802.11n USB Wireless Card"
Amigo_9031.DeviceDesc       = "802.11n Wireless USB Card"
Amigo_9041.DeviceDesc       = "802.11n Wireless USB Card"
PEGATRON_0001.DeviceDesc    = "Microsoft 802.11b/g/n Wireless LAN Mini-USB Device"
PEGATRON_0002.DeviceDesc    = "Ralink RT2770/2720 802.11b/g/n Wireless LAN Mini-USB Device"
LevelOne_0605.DeviceDesc    = "LevelOne WUA-0605 N_Max Wireless USB Adapter"
LevelOne_0615.DeviceDesc    = "LevelOne WUA-0615 N_Max Wireless USB Adapter"
Quanta_0304.DeviceDesc      = "802.11n Wireless LAN Card"
Zinwell_0280.DeviceDesc     = "802.11a/b/g/n USB Wireless LAN Card"
Zinwell_0282.DeviceDesc     = "802.11b/g/n USB Wireless LAN Card"
Logitec_0162.DeviceDesc     = "Logitec LAN-WN22/U2 Wireless LAN Adapter"
Logitec_0163.DeviceDesc     = "Logitec LAN-WN12/U2 Wireless LAN Adapter"
Logitec_0164.DeviceDesc     = "Logitec LAN-WN11/U2 Wireless LAN Adapter"

INSTALL_DISK_STR            = "Wireless 11n USB Installation Disk"

Generic.Service.DispName    = "RT2870 USB Wireless LAN Card Driver for Vista"

;
; Parameters
;
TXBurst                     = "TX Burst"
Disable                     = "Disable"
Enable                      = "Enable"
RadioOnOff                  = "Radio On/Off"
CountryRegion24G            = "Country Region 11G"
CountryRegion24G_0          = "#0 (Channel 1 - 11)"
CountryRegion24G_1          = "#1 (Channel 1 - 13)"
CountryRegion24G_2          = "#2 (Channel 10 - 11)"
CountryRegion24G_3          = "#3 (Channel 10 - 13)"
CountryRegion24G_4          = "#4 (Channel 14)"
CountryRegion24G_5          = "#5 (Channel 1 - 14)"
CountryRegion24G_6          = "#6 (Channel 3 - 9)"
CountryRegion24G_7          = "#7 (Channel 5 - 13)"
CountryRegion5G             = "Country Region 11A"
CountryRegion5G_0           = "#0 Ch(36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 Ch(36 - 140)"
CountryRegion5G_2           = "#2 Ch(36 - 64)"
CountryRegion5G_3           = "#3 Ch(52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 Ch(149 - 165)"
CountryRegion5G_5           = "#5 Ch(149 - 161)"
CountryRegion5G_6           = "#6 Ch(36 - 48)"
CountryRegion5G_7           = "#7 Ch(36 - 165)"
CountryRegion5G_8           = "#8 Ch(52 - 64)"
CountryRegion5G_9           = "#9 Ch(36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 Ch(36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 Ch(36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 Ch(36 - 140)"
RDG                         = "RDG"
WMMCapable                  = "WMM Capable"
HTCapable                   = "HT Capable"
IEEE802_11h                 = "IEEE802.11h"
CarrierDetect               = "Carrier Detect"
SmartScan                   = "SmartScan"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"

